; DSD+ frequency file
;
; you can edit this file while DSD+ is running
;
; line format:
;
;  protocol, networkID, siteNumber, OTAchannelNumber, TXfrequency, RXfrequency, sortOrder
;
;  for TIII, siteNumber format = area.site
;
;
;   use site number = 0 for network-wide definition
;
;   use 0.0 for unknown frequencies
;
;   use sort order = 0 to sort by OTA channel number
;
;
; protocols:
;
;  D-Star
;  IDAS
;  NEXEDGE48
;  NEXEDGE96
;  dPMR
;  DMR
;  Cap+
;  Con+
;  TIII
;  P25
;  ProVoice

